Title: User Story 13 – Revocation of MA

**Objective:**

This operational scenario verifies the reaction of the onboard in case of MA revocation

**Diagram:**



Train is running with an MA beyond SMB204. The MA is revoked by the traffic

control center such that the train is able to stop before the revoked SMB204.